RTCC Timer 0 overflow (using RTCC name)
TIMER0 Timer 0 overflow (using TIMER0 name)
TIMER1 Timer 1 overflow
TIMER2 Timer 2 overflow
TIMER3 Timer 3 overflow
TIMER4 Timer 4 overflow
TIMER5 Timer 5 overflow 
TIMER6 Timer 6 overflow
TIMER7 Timer 7 overflow
TIMER8 Timer 8 overflow
TIMER9 Timer 9 overflow
EXT  External interrupt
EXT0  External interrupt
EXT1 External interrupt #1
EXT2 External interrupt #2
EXT3 External interrupt #3
EXT4 External interrupt #4
OSC_FAIL System oscillator failed
OSCFAIL System oscillator failed 1
ADDRERR Address trror trap 
STACKERR Stack error trap
MATHERR Arithmetic error trap
DMAERR DMAC error trap
RB0  Port B bit 0 change
RB1  Port B bit 0 change
RB2  Port B bit 0 change
RB3  Port B bit 0 change
RB4  Port B bit 0 change
RB5  Port B bit 0 change
RB6  Port B bit 0 change
RB7  Port B bit 0 change
RB   Port B any change on B4-B7
RC   Port C any change on C4-C7
RA   Port A change
T1_CAPT Capture on unit 1
T1_COMP Compare on unit 1
T2_CAPT Capture on unit 2
T2_COMP Compare on unit 2
AD Analog to digital conversion complete
ADOF Analog to digital conversion timeout
TBE RS232 transmit buffer empty
TBE0 RS232 transmit buffer 0 empty
TBE1 RS232 transmit buffer 1 empty
TBE2 RS232 transmit buffer 2 empty
RDA RS232 receive data available
RDA0 RS232 receive data available in buffer 0
RDA1 RS232 receive data available in buffer 1
RDA2 RS232 receive data available in buffer 2
CCP1 Capture or Compare on unit 1
CCP2 Capture or Compare on unit 2
CCP3 Capture or Compare on unit 3
CCP4 Capture or Compare on unit 4
CCP5 Capture or Compare on unit 5
SSP SPI or I2C activity
I2C I2C activity
PSP Parallel Slave Port data in
LCD LCD activity
LVD Low voltage detected
COMP Comparator 1 detect
COMP2 Comparator 2 detect
BUTTON Pushbutton
BUSCOL Bus collision
LOWVOLT Low voltage detected
EEPROM Data eeprom Write complete
USB Universal Serial Bus activity
CANIRX An invalid message has occured on the CAN bus
CANWAKE Bus Activity wake-up has occured on the CAN bus
CANERR An error has occured in the CAN module
CANTX2 CAN Transmit buffer 2 has completed transmission
CANTX1 CAN Transmit buffer 1 has completed transmission
CANTX0 CAN Transmit buffer 0 has completed transmission
CANRX1 CAN Receive buffer 1 has received a new message
CANRX0 CAN Receive buffer 0 has received a new message
OSCF Oscillator fail
BUSCOL2 MSSP2 Bus Collision
SSP2 MSSP2 SPI or I2C activity
PWMTB PWM Time Base
IC3DR IC3/QEI Direction
IC2QEI IC2/QEI 
IC1 IC1/QEI
SPP Streaming Parallel Port Read/Write
CR Cryptographic activity complete
COMP1 Comparator 1 detect
OSCF System oscilator failed
SSP2 SPI or I2C activity for Port 2
USB Universal Serial Bus activity
AC1     Analog comparator 1 output change
AC2     Analog comparator 2 output change
AC3     Analog comparator 3 output change
AC4     Analog comparator 4 output change
AD      Analog to digital conversion complete
AD2     ADC1 conversion complete
ADC1    Analog to digital conversion complete
ADC2    Analog to digital conversion complete
ADCP0   ADC pair 0 conversion complete
ADCP1   ADC pair 1 conversion complete
ADCP2   ADC pair 2 conversion complete
ADCP3   ADC pair 3 conversion complete
ADCP4   ADC pair 4 conversion complete
ADCP5   ADC pair 5 conversion complete
CAN1    CAN 1 Combined Interrupt Request
CAN1E   CAN 1 Event 
CAN1RX  CAN 1 Receive Buffer Ready
CAN1TX  CAN 1 Transmit Data Request
CAN2    CAN 2 Combined Interrupt Request
CAN2E   CAN 2 Event
CAN2RX  CAN 2 Receive Buffer Ready
CAN2TX  CAN 2 Transmit Data Request
COMP    Comparator event
CRC     Cyclic redundancy check generator
DCI     DCI transfer done
DCIE    DCE error
DMA0    DMA channel 0 transfer complete
DMA1    DMA channel 1 transfer complete
DMA2    DMA channel 2 transfer complete
DMA3    DMA channel 3 transfer complete
DMA4    DMA channel 4 transfer complete
DMA5    DMA channel 5 transfer complete
DMA6    DMA channel 6 transfer complete
DMA7    DMA channel 7 transfer complete
EEPROM  Write complete
FAULTA  PWM Fault A
FAULTB  PWM Fault B
IC1     Input Capture #1
IC2     Input Capture #2
IC3     Input Capture #3
IC4     Input Capture #4
IC5     Input Capture #5
IC6     Input Capture #6
IC7     Input Capture #7
IC8     Input Capture #8
ICN     Input change notification interrupt
LOWVOLT	Low voltage detected
MI2C    Master I2C activity
MI2C1   Master1 I2C activity
MI2C2   Master2 I2C activity
NVM     Non-volatile memory write complete
OC1     Output Compare #1
OC2     Output Compare #2
OC3     Output Compare #3
OC4     Output Compare #4
OC5     Output Compare #5
OC6     Output Compare #6
OC7     Output Compare #7
OC8     Output Compare #8
OSC_FAIL System oscillator failed
PMP     Parallel master port
PWM     PWM period match
PWM1    PWM generator 1 time based interrupt
PWM2    PWM generator 2 time based interrupt
PWM3    PWM generator 3 time based interrupt
PWM4    PWM generator 4 time based interrupt
PWMP    PWM 1 period match
PWMP2   PWM 2 period match
PWMSEM  PWM special event trigger
QEI     QEI position counter compare
RDA     RS232 receive data available
RDA2    RS232 receive data available in buffer 2
RTC     Real - Time Clock/Calendar
SI2C    Slave I2C activity
SI2C1   Slave1 I2C activity
SI2C2   Slave2 I2C activity
SPI1    SPI1 Transfer Done
SPI1E   SPI1E Transfer Done
SPI2    SPI2 Transfer Done
SPI2E   SPI2 Error
SPIE    SPI Error
TBE     RS232 transmit buffer empty
TBE2    RS232 transmit buffer 2 empty
UART1E  UART1 error
UART2E  UART2 error
CHANGE  Change notice interrupt 
CNI     Change notice interrupt
	